ssid=KV-800SH_0605
hw_mode=g
channel=6
interface=wlan0
bridge=br0
driver=rtl871xdrv
ignore_broadcast_ssid=0
macaddr_acl=0
beacon_int=100
ieee80211n=1
ht_capab=[SHORT-GI-20][SHORT-GI-40][HT40+]
max_num_sta=5
#wpa=2
#wpa_passphrase=11111111
#wpa_key_mgmt=WPA-PSK
#wpa_pairwise=CCMP
